**WARRANTY:**  There is a full 2 year Parts and Labour Warranty on the Vinetech Birdscarer. Any liability or claim against Vinetech shall not exceed the purchase price.


NOTE: Remove battery at the end of the season.

*The effectiveness of this device will be improved with shotgun backup*

**VINETECH**

Electronic

Birdscarer



INSTRUCTION MANUAL

Assembly and operation


*Vinetech*

*Electronic*

*Birdscarer*

IMPORTANT

Read before use



**AVAILABLE ACCESSORIES**

Spare rechargeable batteries

Solar panel charging option

**SAFETY PRECAUTIONS**

* DO NOT operate birdscarer where surrounding materials may catch fire
* Use LPG only
* Operate birdscarer in an open area
* Ensure legs are on stable ground to prevent tipping over.
* Frequently check barrel for obstructions and clear if necessary.
* Never operate the birdscarer without spark plug leads connected otherwise damage to the circuit board could occur.
* Always wear hearing protection when in the vicinity of an operating birdscarer

**For further information contact:**

Vinetech Birdscarers

Unit 4, 602 Omahu Road

Hastings, 4120

Ph: 027 3897651 email: enquiries@vinetechbirdscarers.com